# Stomp 1.1 Example

    To run the example, simply type mvn verify from this directory,
    or mvn -PnoServer verify if you want to start and create the server manually.

This example shows you how to configure ActiveMQ Artemis to send and receive Stomp messages using Stomp 1.1 protocol.

The example will start a ActiveMQ Artemis server configured with Stomp and JMS.

The client will open a socket to initiate a Stomp 1.1 connection and then send one Stomp message (using TCP directly). The client will then consume a message from a JMS Queue and check it is the message sent with Stomp.